{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Piling","Format","Comments"],"read":"whole","date_system":"1900"}

{"sheet":"Piling","index":0,"n_rows":5,"n_cols":6,"rows_kept":5}
[null,null,"Precast Concrete Pile"]
[null,null,"Introduction and Site Organisation ( All Provisional except where stated otherwise"]
["A",null,"Information of soil condition and of the bore holes put down over the site, together with results of laboratory tests on samples of soil from the bore holes may be inspected at the office of Engineer during normal office hour.","Item",1,0]
["B",null,"If the Tenderers wish to carry out any further tests on the site they may do so at their own expenses after obtaining permission from the Architect.","Item",1,0]
[null,null,"Allow for Working load testing on single 175 x 175mm Precast Concrete piles to a working load of 350KN.","No.",3,5000]

{"sheet":"Format","index":1,"n_rows":2,"n_cols":8,"rows_kept":2,"merged":[[0,4,0,5],[0,6,0,7]]}
[{"$nulls":4},"Budget",null,"Sub con"]
[null,null,"Descrption","Unit","  QTY","  Rate","  QTY","  Rate"]

{"sheet":"Comments","index":2,"n_rows":2,"n_cols":1,"rows_kept":2}
["Prefer can mark and delete"]
["Prefer can use 2010 version excel"]